|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Fond-Rec_e | | **International Telecommunication Union** | | |
|  | |  | | |
| **ITU-T** | **G.711** | |
| TELECOMMUNICATION STANDARDIZATION SECTOR OF ITU | | **Amendment 2**  (11/2009) |
|  | SERIES G: TRANSMISSION SYSTEMS AND MEDIA, DIGITAL SYSTEMS AND NETWORKS  Digital terminal equipments – Coding of voice and audio signals | | | |
|  | Pulse code modulation (PCM) of voice frequencies  **Amendment 2: New Appendix III – Audio quality enhancement toolbox** | | | |
|  | Recommendation ITU‑T G.711 (1988)  – Amendment 2 | | | |



ITU-T G-SERIES RECOMMENDATIONS

**TRANSMISSION SYSTEMS AND MEDIA, DIGITAL SYSTEMS AND NETWORKS**

|  |  |
| --- | --- |
|  |  |
| INTERNATIONAL TELEPHONE CONNECTIONS AND CIRCUITS | G.100–G.199 |
| GENERAL CHARACTERISTICS COMMON TO ALL ANALOGUE CARRIER-TRANSMISSION SYSTEMS | G.200–G.299 |
| INDIVIDUAL CHARACTERISTICS OF INTERNATIONAL CARRIER TELEPHONE SYSTEMS ON METALLIC LINES | G.300–G.399 |
| GENERAL CHARACTERISTICS OF INTERNATIONAL CARRIER TELEPHONE SYSTEMS ON RADIO-RELAY OR SATELLITE LINKS AND INTERCONNECTION WITH METALLIC LINES | G.400–G.449 |
| COORDINATION OF RADIOTELEPHONY AND LINE TELEPHONY | G.450–G.499 |
| TRANSMISSION MEDIA AND OPTICAL SYSTEMS CHARACTERISTICS | G.600–G.699 |
| DIGITAL TERMINAL EQUIPMENTS | G.700–G.799 |
| General | G.700–G.709 |
| **Coding of voice and audio signals** | **G.710–G.729** |
| Principal characteristics of primary multiplex equipment | G.730–G.739 |
| Principal characteristics of second order multiplex equipment | G.740–G.749 |
| Principal characteristics of higher order multiplex equipment | G.750–G.759 |
| Principal characteristics of transcoder and digital multiplication equipment | G.760–G.769 |
| Operations, administration and maintenance features of transmission equipment | G.770–G.779 |
| Principal characteristics of multiplexing equipment for the synchronous digital hierarchy | G.780–G.789 |
| Other terminal equipment | G.790–G.799 |
| DIGITAL NETWORKS | G.800–G.899 |
| DIGITAL SECTIONS AND DIGITAL LINE SYSTEM | G.900–G.999 |
| MULTIMEDIA QUALITY OF SERVICE AND PERFORMANCE – GENERIC AND USER-RELATED ASPECTS | G.1000–G.1999 |
| TRANSMISSION MEDIA CHARACTERISTICS | G.6000–G.6999 |
| DATA OVER TRANSPORT – GENERIC ASPECTS | G.7000–G.7999 |
| PACKET OVER TRANSPORT ASPECTS | G.8000–G.8999 |
| ACCESS NETWORKS | G.9000–G.9999 |
|  |  |

*For further details, please refer to the list of ITU-T Recommendations.*

|  |
| --- |
| Recommendation ITU-T G.711  Pulse code modulation (PCM) of voice frequencies  Amendment 2  New Appendix III – Audio quality enhancement toolbox |

|  |
| --- |
| Summary  Appendix III to ITU-T Recommendation G.711 describes a toolbox to provide audio quality enhancements to ITU-T G.711. The toolbox comprises four tools that are algorithms initially developed in the context of ITU-T G.711.1 wideband speech and audio codec.  The four tools aim at enhancing the quality of ITU-T G.711 legacy for both encoder and decoder sides. At the encoder side is a noise shaping tool which is used in combination with a modified ITU‑T G.711 encoder to perceptually shape the coding noise of the PCM encoder and produce a compatible bit stream. At the decoder, the three tools offer an improved audio quality and/or a better robustness against packet losses. The first tool is a noise gate which is used to increase the clearness of the audio signal during quasi-silent periods. The second tool is a postfilter which reduces the PCM quantization noise of legacy ITU-T G.711. The third is a frame erasure concealment algorithm which is used to extrapolate the signal in case of erased frames. The toolbox has been tested with a frame size of 5 ms. The overall complexity of the toolbox is about 4 WMOPS.  All of these tools can be used separately or in combination.  This appendix contains an electronic attachment containing the respective ANSI-C source code. |

|  |
| --- |
| Source  Amendment 2 to Recommendation ITU‑T G.711 (1988) was agreed on 6 November 2009 by ITU‑T Study Group 16 (2009-2012). |

|  |
| --- |
|  |

FOREWORD

The International Telecommunication Union (ITU) is the United Nations specialized agency in the field of tele­com­mu­ni­ca­tions, information and communication technologies (ICTs). The ITU Telecommunication Standardization Sector (ITU-T) is a permanent organ of ITU. ITU-T is responsible for studying technical, operating and tariff questions and issuing Recommendations on them with a view to standardizing telecommunications on a worldwide basis.

The World Telecommunication Standardization Assembly (WTSA), which meets every four years, establishes the topics for study by the ITU‑T study groups which, in turn, produce Recommendations on these topics.

The approval of ITU-T Recommendations is covered by the procedure laid down in WTSA Resolution 1.

In some areas of information technology which fall within ITU-T's purview, the necessary standards are prepared on a collaborative basis with ISO and IEC.

NOTE

In this Recommendation, the expression "Administration" is used for conciseness to indicate both a telecommunication administration and a recognized operating agency.

Compliance with this Recommendation is voluntary. However, the Recommendation may contain certain mandatory provisions (to ensure e.g. interoperability or applicability) and compliance with the Recommendation is achieved when all of these mandatory provisions are met. The words "shall" or some other obligatory language such as "must" and the negative equivalents are used to express requirements. The use of such words does not suggest that compliance with the Recommendation is required of any party.

INTELLECTUAL PROPERTY RIGHTS

ITU draws attention to the possibility that the practice or implementation of this Recommendation may involve the use of a claimed Intellectual Property Right. ITU takes no position concerning the evidence, validity or applicability of claimed Intellectual Property Rights, whether asserted by ITU members or others outside of the Recommendation development process.

As of the date of approval of this Recommendation, ITU had received notice of intellectual property, protected by patents, which may be required to implement this Recommendation. However, implementers are cautioned that this may not represent the latest information and are therefore strongly urged to consult the TSB patent database at [http://www.itu.int/ITU-T/ipr/.](http://www.itu.int/ITU-T/ipr/)

©  ITU  2010

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without the prior written permission of ITU.

**CONTENTS**

Page

III.1 Scope 1

III.2 References 1

III.3 Definitions 1

III.4 Abbreviations and acronyms 1

III.5 Conventions 2

III.6 General description of the toolbox 2

III.7 Functional description of the toolbox for the encoder 4

III.8 Functional description of the toolbox for the decoder 4

III.9 Bit-exact description of the audio quality enhancement toolbox for ITU‑T G.711 5

Electronic attachment: ANSI-C source code.

Recommendation ITU-T G.711

Pulse code modulation (PCM) of voice frequencies

Amendment 2  
  
New Appendix III – Audio quality enhancement toolbox[[1]](#footnote-1)

## III.1 Scope

This appendix contains the description of a toolbox to provide audio quality enhancements to the legacy ITU-T G.711 codec.

This appendix is organized as follows. The references, definitions, abbreviations and acronyms, and conventions used throughout this appendix are defined in clauses III.2, III.3, III.4, and III.5, respectively. Clause III.6 gives a general outline of the four algorithms. The noise shaping (NS) is discussed in clause III.7.1. The frame erasure concealment (FERC) is presented in clause III.8.1. The noise gate (NG) and the postfilter (PF) are described in clauses III.8.2 and III.8.3, respectively. Clause III.9 describes the software that defines this toolbox in 16-32-bit fixed-point arithmetic.

## III.2 References

– ITU-T Recommendation G.191 (2005), *Software tools for speech and audio coding standardization*.

– ITU-T Recommendation G.192 (1996), *A common digital parallel interface for speech standardization activities*.

– ITU-T Recommendation G.711.1 (2008), *Wideband embedded extension for G.711 pulse code modulation*.

## III.3 Definitions

This clause is intentionally left blank.

## III.4 Abbreviations and acronyms

This appendix uses the abbreviations and acronyms listed in Table III.1.

Table III.1 – Glossary of abbreviations and acronyms

| Acronym | Description |
| --- | --- |
| FERC | Frame Erasure Concealment |
| NB | Narrow-Band |
| NG | Noise Gate |
| NS | Noise Shaping |
| PCM | Pulse Code Modulation |
| PF | PostFilter |
| WMOPS | Weighted Millions of Operations Per Second |

## III.5 Conventions

Time-domain signals are denoted by their symbol and a sample index between parentheses, e.g., *s*(*n*). The variable *n* is used as sample index.

Table III.2 lists the most relevant symbols used throughout this appendix.

Table III.2 – Glossary of most relevant symbols

| Type | Name | Description |
| --- | --- | --- |
| Filters |  | Perceptual weighting filter |
| Signals |  | Input signal |
|  | Pre-processed input signal |
|  | Perceptually weighted target signal |
|  | Difference signal of  and |
|  | Decoded signal of ITU-T G.711 bit stream, without offset |
|  | Decoded signal of ITU-T G.711 |
|  | Signal after decoding and FERC |
|  | Signal after postfilter |
|  | Signal after noise gate |
| Parameters |  | Encoder offset value |
|  | LP coefficient of the perceptual filter |
|  | ITU-T G.711 compatible bit stream |

## III.6 General description of the toolbox

This toolbox contains four algorithms for audio quality enhancement of the legacy ITU-T G.711. The noise shaping (NS) is applied only in the encoder, the frame erasure concealment (FERC), the noise gate (NG) and the postfilter (PF) are applied only in the decoder. These algorithms have been extracted from ITU-T G.711.1 scalable coder/decoder and can be used with ITU-T G.711 legacy coder/decoder. The tools may be used separately or in combination. This toolbox is implemented in fixed point using basic operators version 2.2 defined in the ITU-T G.191 software tool library. This appendix provides a detailed description of all four algorithms.

### III.6.1 Tools for ITU-T G.711 encoder

Only one tool is applied in the encoder: the noise shaping (NS) tool. Figure III.1 shows the high‑level block diagram of an ITU-T G.711 encoder with the NS tool. Figure III.1 is described in detail in clause III.7.



Figure III.1 – High-level block diagram of the noise shaping tool

### III.6.2 Tools for ITU-T G.711 decoder

Figure III.2 shows a high-level block diagram of an ITU-T G.711 decoder combined with three tools: the frame erasure concealment (FERC), the noise gate (NG) and the postfilter (PF). This figure illustrates the recommended execution order of the tools when they are combined.



Figure III.2 – High-level block diagram of decoder toolbox

### III.6.3 Algorithmic delay

Table III.3 gives the algorithmic delay of each tool and the algorithmic delay for the combination of the three tools at the decoder side. Note that these algorithmic delays are given for 5 ms frame size.

Table III.3 – Algorithmic delay of the toolbox (ms)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NS | NG | PF | FERC | FERC+PF+NG |
| 0 | 0 | 2 | 5 | 5 |

### III.6.4 Computational complexity and storage requirements

The observed worst-case complexity of the toolbox is based on the implementation with basic operators of the ITU-T software tool library STL2005 v2.2 in ITU-T G.191. The worst computational complexity is detailed in Table III.4, and all the figures show the observed worst complexity either in μ-law or A-law. The storage requirements in 16-bit words for the four tools are given in Tables III.5. Note that the RAM figures are based on the arrays which form the dominant part, but not on singular variables. It was found that the number of such variables was insignificant when compared with size required by arrays.

Table III.4 – Worst computational complexity of the toolbox [WMOPS]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NS | NG | PF | FERC | FERC+PF+NG |
| 0.87 | 0.23 | 2.02 | 2.05 | 3.31 |

Table III.5 – Storage requirements of the toolbox

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Memory type | NS | NG | PF | FERC |
| Static RAM (kWords) | 0.093 | 0.003 | 0.353 | 0.984 |
| Scratch RAM (kWords) | 0.107 | 0.012 | 0.529 | 0.314 |
| Data ROM (kWords) | 0.088 | 0 | 0.191 | 0.121 |
| Program ROM (number of basic ops) | 191 | 37 | 593 | 728 |

### III.6.5 Toolbox description

The description of the toolbox algorithms is made in terms of bit-exact fixed-point mathematical operations. The ANSI-C code indicated in clause III.9, which constitutes an integral part of this appendix, reflects this bit-exact, fixed-point descriptive approach. The mathematical descriptions of the encoder and decoder can be implemented in other fashions, possibly leading to a codec implementation not complying with this appendix. Therefore, the algorithm description of the ANSI‑code of clause III.9 shall take precedence over the mathematical descriptions whenever discrepancies are found.

## III.7 Functional description of the toolbox for the encoder

### III.7.1 Noise shaping (NS) tool

The input signal *sNB*(*n*) is encoded using µ*-*law or A*-*law pulse code modulation (PCM) with noise feedback to perceptually shape the coding noise of the PCM encoder. The encoder with weighted noise feedback loop is shown in Figure III.1. First, the input signal *sNB*(*n*) is pre-processed by a high-pass filter with a cut-off frequency of 50 Hz. Then, the pre-processed signal *sLB*(*n*) is added to a noise feedback signal and the offset value *cLoff*, and the resulting signal *s*'*LB*(*n*) is fed to the legacy ITU‑T G.711 encoder. Based on the obtained bit stream *IL*0(n) the legacy ITU-T G.711 decoder locally decodes the signal *ŝL*0(*n*) and the offset value *cLoff* is removed to obtain *ŝ*'*L*0(*n*). An LP analysis is then performed on *ŝ*'*L*0(*n*) to obtain the coefficients *ai*, and the perceptual filter *F*(*z*) is calculated. Then the quantization noise *dL*0(*n*), filtered by *F*(*z*), is fed back to be added to the input signal s*LB*(*n*). It should be noted that for very low energy signals, the legacy ITU-T G.711 encoding, based on log-PCM, is replaced by a different encoding scheme called "dead-zone quantizer". This is described later in clause III.7.1.4.

#### III.7.1.1 Pre-processing high-pass filter

Same as clause 7.1 of ITU-T G.711.1.

#### III.7.1.2 PCM encoder based on G.711

Same as clause 7.3.1 of ITU-T G.711.1.

#### III.7.1.3 Perceptual filtering

Same as clause 7.3.2 of ITU-T G.711.1.

#### III.7.1.4 Dead-zone quantizer

Same as clause 7.3.3 of ITU-T G.711.1.

## III.8 Functional description of the toolbox for the decoder

The toolbox includes three tools at the decoder side. All these tools can be used either in combination or alone. Figure III.2 describes the tool position in the processing chain. The algorithmic descriptions of the tools are given in the following clauses.

### III.8.1 Narrow-band frame erasure concealment (FERC)

Same as clause 8.4 of ITU-T G.711.1.

### III.8.2 Noise gate (NG)

Same as clause 8.7 of ITU-T G.711.1.

### III.8.3 Postfilter (PF)

Same as Appendix I of ITU-T G.711.1.

## III.9 Bit-exact description of the audio quality enhancement toolbox for ITU-T G.711

The ANSI-C code simulating the audio quality enhancement toolbox in 16-bit fixed-point is available as an electronic attachment to this appendix. The following subclauses summarize the use of this simulation code, and how the software is organized.

### III.9.1 Use of the simulation software

The C code consists of two main programs, encoder.c and decoder.c which simulate the toolbox for encoder and decoder, respectively.

The command line for the encoder is as follows:

**encoder [-options] <law> <infile> <codefile>**

where

|  |  |
| --- | --- |
| law | is the desired ITU-T G.711 law (A or μ) |
| infile | is the name of the input file to be encoded |
| codefile | is the name of the output bit stream file |
| options: | |
| -ns | indicates that noise shaping tool is activated |
| -hardbit | output bit stream file is in multiplexed hardbit format |
| -quiet | quiet processing |

The command line for the decoder is as follows:

**decoder [-options] <law> <codefile> <outfile>**

where

|  |  |
| --- | --- |
| law | is the desired ITU-T G.711 law (A or μ) |
| codefile | is the name of the input bit stream file |
| outfile | is the name of the decoded output file |
| options: |  |
| -ng | indicates that noise gate tool is activated |
| -pf | indicates that postfilter tool is activated |
| -ferc | indicates that frame erasure concealment tool is activated |
| -hardbit | input bit stream file is in multiplexed hardbit format |
| -quiet | quiet processing |

The encoder input and the decoder output files are sampled data files containing 16-bit PCM signals. The encoder output and decoder input files follow the ITU-T G.192 bit stream format by default. The frame erasure can only be simulated with the ITU-T G.192 bit stream format.

### III.9.2 Organization of the simulation software

Tables III.6 to III.9 describe the organization of the simulation software.

Table III.6 – Tables in C-code

| Table name | Symbol | Size | Format | Description |
| --- | --- | --- | --- | --- |
| NS\_window |  | 80 | Q15 | LPC analysis window for noise shaping |
| NS\_lag\_h |  | 4 | Q15 | Lag windowing for noise shaping (MSB of double precision format) |
| NS\_lag\_l | 4 | Q16 | Lag windowing for noise shaping (LSB of double precision format) |
| LBFEC\_lag\_h |  | 16 | Q15 | Lag windowing for FERC (MSB and LSB of double precision format) |
| LBFEC\_lag\_l | 16 | Q16 | Lag windowing for FERC (LSB of double precision format) |
| LBFEC\_lpc\_win\_80 |  | 80 | Q15 | LPC analysis window for FERC |
| LBFEC\_fir\_lp |  | 9 | Q16 | FIR decimation filter coefficients in FERC |
| max\_err\_quant |  | 16 | Q0 | A-law quantization step size |
| Hann\_sh16 |  | 64 | Q15 | Asymmetric Hanning window (for 64-point FFT processing) |
| Hann\_sh16\_p6 |  | 7 | Q15 | Half of 16-point Hanning window for filter interpolation |
| Hann\_sh16\_p6m1 |  | 7 | Q15 | Complementary half of Hanning window for filter interpolation |
| WinFilt |  | 17 | Q15 | Truncating window for impulse response of noise reduction filter |

Table III.7 – Summary of specific routines for encoder toolbox

| Filename | Description |
| --- | --- |
| encoder.c | ITU-T G.711 toolbox encoder interface |
| G711Appenc.c | ITU-T G.711 toolbox main encoder |
| prehpf.c | High-pass pre-filter |
| lowband\_enc.c | Encoder toolbox |

Table III.8 – Summary of specific routines for decoder toolbox

| Filename | Description |
| --- | --- |
| decoder.c | ITU-T G.711 toolbox decoder interface |
| g711Appdec.c | ITU-T G.711 toolbox main decoder |
| fec\_lowband.c | Frame erasure concealment (FERC) |
| lowband\_dec.c | Decoder toolbox |
| post.c | Main routine that calls all post-processing subroutines |
| post\_anasyn.c | Analysis/synthesis subroutines for post-processing |
| post\_gainfct.c | Subroutines for estimating of the post-processing filter |
| post\_rfft.c | 64-point real FFT and ifft |
| table\_post.c | Tables for postfilter |

Table III.9 – Summary of common routines

| Filename | Description |
| --- | --- |
| softbit.c | Conversion between hardbit and softbit |
| autocorr\_ns.c | Autocorrelation of signal for noise shaping |
| g711a.c | PCM coder and decoder (A-law) |
| g711mu.c | PCM coder and decoder (μ-law) |
| lpctools.c | Linear prediction tools |
| table\_lowband.c | Tables for lower-band modules |
| dsputil.c | Fixed-point utility routines |
| errexit.c | Exit routine |
| mathtool.c | Square-root routines |
| oper\_32b.c | Basic operators in double precision (32 bits) |
| table\_mathtool.c | Tables for square-root routines |

|  |  |
| --- | --- |
| **SERIES OF ITU-T RECOMMENDATIONS** | |
| Series A | Organization of the work of ITU-T |
| Series D | General tariff principles |
| Series E | Overall network operation, telephone service, service operation and human factors |
| Series F | Non-telephone telecommunication services |
| **Series G** | **Transmission systems and media, digital systems and networks** |
| Series H | Audiovisual and multimedia systems |
| Series I | Integrated services digital network |
| Series J | Cable networks and transmission of television, sound programme and other multimedia signals |
| Series K | Protection against interference |
| Series L | Construction, installation and protection of cables and other elements of outside plant |
| Series M | Telecommunication management, including TMN and network maintenance |
| Series N | Maintenance: international sound programme and television transmission circuits |
| Series O | Specifications of measuring equipment |
| Series P | Terminals and subjective and objective assessment methods |
| Series Q | Switching and signalling |
| Series R | Telegraph transmission |
| Series S | Telegraph services terminal equipment |
| Series T | Terminals for telematic services |
| Series U | Telegraph switching |
| Series V | Data communication over the telephone network |
| Series X | Data networks, open system communications and security |
| Series Y | Global information infrastructure, Internet protocol aspects and next-generation networks |
| Series Z | Languages and general software aspects for telecommunication systems |
|  |  |

1. This appendix includes an electronic attachment containing the respective ANSI-C source code. [↑](#footnote-ref-1)